|  |  |
| --- | --- |
| General | |
| Physical dimensions | 4.8"W x 3.0"H x .8"D (12.2 x 7.6 x 2.0 cm) |
| Weight | 6.48 ounces (183.8 g) |
| Battery | rechargeable lithium-ion |
| Display type | WQVGA color TFT with white backlight |
| Display size | 3.81"W x 2.25"H (9.7 x 5.7 cm); 4.3" diag (10.9 cm) |
| Display resolution | 480 x 272 pixels |
| Battery life | up to 3 hours |

|  |  |
| --- | --- |
| Maps & Memory | |
| Preloaded street maps |  |
| Storage and Power Capacity | SD™ card (not included) |
| 3-D buildings and landmarks view |  |

|  |  |
| --- | --- |
| Navigation Features | |
| Traffic compatible | Yes (receiver and lifetime traffic included) |
| Lifetime traffic updates |  |
| Lane assist with junction view (displays junction signs) |  |
| Bluetooth® calling | Yes (with A2DP technology) |
| Speed limit indicator (displays speed limit for most major roads in the U.S. and Europe) |  |
| MP3 player |  |

|  |  |
| --- | --- |
| Semi Truck Features | |
| Headphone jack/audio line-out |  |

|  |  |
| --- | --- |
| Additional | |
| Additional | This USB mass storage device is compatible with Windows® XP or newer and Mac® OS X 10.4 or later. |